Understanding Arducopter code:

wp\_nav function used to set waypoints (might be useful) appears in navigation

control mode variable used to set the flight mode(acro alt hold ect) appears in events

radio.ino Function that will read the radio data in radio

read\_me.text describes how the serial inp and out should work.

Setup.ino function that deals with serial functions. I/O